/*
WARNING: Do NOT edit the input and output ports in this file in a text
editor if you plan to continue editing the block that represents it in
the Block Editor! File corruption is VERY likely to occur.
*/
/*
Copyright (C) 2016  Intel Corporation. All rights reserved.
Your use of Intel Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Intel Program License 
Subscription Agreement, the Intel Quartus Prime License Agreement,
the Intel MegaCore Function License Agreement, or other 
applicable license agreement, including, without limitation, 
that your use is for the sole purpose of programming logic 
devices manufactured by Intel and sold by Intel or its 
authorized distributors.  Please refer to the applicable 
agreement for further details.
*/
(header "symbol" (version "1.1"))
(symbol
	(rect 16 16 352 288)
	(text "top_control" (rect 5 0 48 12)(font "Arial" ))
	(text "inst" (rect 8 256 20 268)(font "Arial" ))
	(port
		(pt 0 32)
		(input)
		(text "dcm_96MHz" (rect 0 0 51 12)(font "Arial" ))
		(text "dcm_96MHz" (rect 21 27 72 39)(font "Arial" ))
		(line (pt 0 32)(pt 16 32)(line_width 1))
	)
	(port
		(pt 0 48)
		(input)
		(text "reset" (rect 0 0 20 12)(font "Arial" ))
		(text "reset" (rect 21 43 41 55)(font "Arial" ))
		(line (pt 0 48)(pt 16 48)(line_width 1))
	)
	(port
		(pt 0 64)
		(input)
		(text "fpga_receive" (rect 0 0 53 12)(font "Arial" ))
		(text "fpga_receive" (rect 21 59 74 71)(font "Arial" ))
		(line (pt 0 64)(pt 16 64)(line_width 1))
	)
	(port
		(pt 0 80)
		(input)
		(text "spi_data[15..0]" (rect 0 0 56 12)(font "Arial" ))
		(text "spi_data[15..0]" (rect 21 75 77 87)(font "Arial" ))
		(line (pt 0 80)(pt 16 80)(line_width 3))
	)
	(port
		(pt 0 96)
		(input)
		(text "adc_ready" (rect 0 0 43 12)(font "Arial" ))
		(text "adc_ready" (rect 21 91 64 103)(font "Arial" ))
		(line (pt 0 96)(pt 16 96)(line_width 1))
	)
	(port
		(pt 0 112)
		(input)
		(text "sin_data[11..0]" (rect 0 0 55 12)(font "Arial" ))
		(text "sin_data[11..0]" (rect 21 107 76 119)(font "Arial" ))
		(line (pt 0 112)(pt 16 112)(line_width 3))
	)
	(port
		(pt 0 128)
		(input)
		(text "cos_data[11..0]" (rect 0 0 59 12)(font "Arial" ))
		(text "cos_data[11..0]" (rect 21 123 80 135)(font "Arial" ))
		(line (pt 0 128)(pt 16 128)(line_width 3))
	)
	(port
		(pt 0 144)
		(input)
		(text "lisa_counter[15..0]" (rect 0 0 70 12)(font "Arial" ))
		(text "lisa_counter[15..0]" (rect 21 139 91 151)(font "Arial" ))
		(line (pt 0 144)(pt 16 144)(line_width 3))
	)
	(port
		(pt 0 160)
		(input)
		(text "mcu2fpga_spi_done" (rect 0 0 81 12)(font "Arial" ))
		(text "mcu2fpga_spi_done" (rect 21 155 102 167)(font "Arial" ))
		(line (pt 0 160)(pt 16 160)(line_width 1))
	)
	(port
		(pt 0 176)
		(input)
		(text "fpga2mcu_spi_done" (rect 0 0 81 12)(font "Arial" ))
		(text "fpga2mcu_spi_done" (rect 21 171 102 183)(font "Arial" ))
		(line (pt 0 176)(pt 16 176)(line_width 1))
	)
	(port
		(pt 0 192)
		(input)
		(text "inc_lut_dout[7..0]" (rect 0 0 67 12)(font "Arial" ))
		(text "inc_lut_dout[7..0]" (rect 21 187 88 199)(font "Arial" ))
		(line (pt 0 192)(pt 16 192)(line_width 3))
	)
	(port
		(pt 0 208)
		(input)
		(text "quotient[8..0]" (rect 0 0 49 12)(font "Arial" ))
		(text "quotient[8..0]" (rect 21 203 70 215)(font "Arial" ))
		(line (pt 0 208)(pt 16 208)(line_width 3))
	)
	(port
		(pt 0 224)
		(input)
		(text "inc_interpolation_result_p01um_done" (rect 0 0 145 12)(font "Arial" ))
		(text "inc_interpolation_result_p01um_done" (rect 21 219 166 231)(font "Arial" ))
		(line (pt 0 224)(pt 16 224)(line_width 1))
	)
	(port
		(pt 0 240)
		(input)
		(text "inc_interpolation_result[10..0]" (rect 0 0 112 12)(font "Arial" ))
		(text "inc_interpolation_result[10..0]" (rect 21 235 133 247)(font "Arial" ))
		(line (pt 0 240)(pt 16 240)(line_width 3))
	)
	(port
		(pt 336 32)
		(output)
		(text "comm_voltage[11..0]" (rect 0 0 82 12)(font "Arial" ))
		(text "comm_voltage[11..0]" (rect 233 27 315 39)(font "Arial" ))
		(line (pt 336 32)(pt 320 32)(line_width 3))
	)
	(port
		(pt 336 48)
		(output)
		(text "ram_wren" (rect 0 0 41 12)(font "Arial" ))
		(text "ram_wren" (rect 274 43 315 55)(font "Arial" ))
		(line (pt 336 48)(pt 320 48)(line_width 1))
	)
	(port
		(pt 336 64)
		(output)
		(text "ram_addr[11..0]" (rect 0 0 62 12)(font "Arial" ))
		(text "ram_addr[11..0]" (rect 253 59 315 71)(font "Arial" ))
		(line (pt 336 64)(pt 320 64)(line_width 3))
	)
	(port
		(pt 336 80)
		(output)
		(text "ram_data[15..0]" (rect 0 0 62 12)(font "Arial" ))
		(text "ram_data[15..0]" (rect 253 75 315 87)(font "Arial" ))
		(line (pt 336 80)(pt 320 80)(line_width 3))
	)
	(port
		(pt 336 96)
		(output)
		(text "start" (rect 0 0 17 12)(font "Arial" ))
		(text "start" (rect 298 91 315 103)(font "Arial" ))
		(line (pt 336 96)(pt 320 96)(line_width 1))
	)
	(port
		(pt 336 112)
		(output)
		(text "resolution[4..0]" (rect 0 0 57 12)(font "Arial" ))
		(text "resolution[4..0]" (rect 258 107 315 119)(font "Arial" ))
		(line (pt 336 112)(pt 320 112)(line_width 3))
	)
	(port
		(pt 336 128)
		(output)
		(text "inc_lut_data_in[7..0]" (rect 0 0 79 12)(font "Arial" ))
		(text "inc_lut_data_in[7..0]" (rect 236 123 315 135)(font "Arial" ))
		(line (pt 336 128)(pt 320 128)(line_width 3))
	)
	(port
		(pt 336 144)
		(output)
		(text "inc_lut_ram_addr[8..0]" (rect 0 0 90 12)(font "Arial" ))
		(text "inc_lut_ram_addr[8..0]" (rect 225 139 315 151)(font "Arial" ))
		(line (pt 336 144)(pt 320 144)(line_width 3))
	)
	(port
		(pt 336 160)
		(output)
		(text "inc_lut_ram_wren" (rect 0 0 71 12)(font "Arial" ))
		(text "inc_lut_ram_wren" (rect 244 155 315 167)(font "Arial" ))
		(line (pt 336 160)(pt 320 160)(line_width 1))
	)
	(port
		(pt 336 176)
		(output)
		(text "test_out_1" (rect 0 0 41 12)(font "Arial" ))
		(text "test_out_1" (rect 274 171 315 183)(font "Arial" ))
		(line (pt 336 176)(pt 320 176)(line_width 1))
	)
	(drawing
		(rectangle (rect 16 16 320 256)(line_width 1))
	)
)
