##
Sample behavioral waveforms for design file "accum.v"

The following waveforms show the behavior of altaccumulate megafunction for the chosen set of parameters in design "accum.v". The design "accum.v" is a 26 bit UNSIGNED accumulator. Data input to the accumulator is of width 19. The accumulator has a synchronous load port to load the data input directly to the accumulator.

Fig. 1 : Wave showing altaccumulate operation.