--Copyright (C) 2016  Intel Corporation. All rights reserved.
--Your use of Intel Corporation's design tools, logic functions 
--and other software and tools, and its AMPP partner logic 
--functions, and any output files from any of the foregoing 
--(including device programming or simulation files), and any 
--associated documentation or information are expressly subject 
--to the terms and conditions of the Intel Program License 
--Subscription Agreement, the Intel Quartus Prime License Agreement,
--the Intel MegaCore Function License Agreement, or other 
--applicable license agreement, including, without limitation, 
--that your use is for the sole purpose of programming logic 
--devices manufactured by Intel and sold by Intel or its 
--authorized distributors.  Please refer to the applicable 
--agreement for further details.


component ram_1
	PORT
	(
		address		: IN STD_LOGIC_VECTOR (11 DOWNTO 0);
		clock		: IN STD_LOGIC  := '1';
		data		: IN STD_LOGIC_VECTOR (15 DOWNTO 0);
		wren		: IN STD_LOGIC ;
		q		: OUT STD_LOGIC_VECTOR (15 DOWNTO 0)
	);
end component;
