<?xml version="1.0" encoding="UTF-8"?>
<system name="$${FILENAME}">
 <component
   name="$${FILENAME}"
   displayName="$${FILENAME}"
   version="1.0"
   description=""
   tags="INTERNAL_COMPONENT=true"
   categories="System" />
 <parameter name="bonusData"><![CDATA[bonusData 
{
   element fft_ii_0
   {
      datum _sortIndex
      {
         value = "0";
         type = "int";
      }
   }
}
]]></parameter>
 <parameter name="clockCrossingAdapter" value="HANDSHAKE" />
 <parameter name="device" value="EP4CE10F17C8" />
 <parameter name="deviceFamily" value="Cyclone IV E" />
 <parameter name="deviceSpeedGrade" value="8" />
 <parameter name="fabricMode" value="QSYS" />
 <parameter name="generateLegacySim" value="false" />
 <parameter name="generationId" value="0" />
 <parameter name="globalResetBus" value="false" />
 <parameter name="hdlLanguage" value="VERILOG" />
 <parameter name="hideFromIPCatalog" value="true" />
 <parameter name="lockedInterfaceDefinition" value="" />
 <parameter name="maxAdditionalLatency" value="1" />
 <parameter name="projectName" value="fft_1024.qpf" />
 <parameter name="sopcBorderPoints" value="false" />
 <parameter name="systemHash" value="0" />
 <parameter name="testBenchDutName" value="" />
 <parameter name="timeStamp" value="0" />
 <parameter name="useTestBenchNamingPattern" value="false" />
 <instanceScript></instanceScript>
 <interface name="clk" internal="fft_ii_0.clk" type="clock" dir="end">
  <port name="clk" internal="clk" />
 </interface>
 <interface name="rst" internal="fft_ii_0.rst" type="reset" dir="end">
  <port name="reset_n" internal="reset_n" />
 </interface>
 <interface name="sink" internal="fft_ii_0.sink" type="conduit" dir="end">
  <port name="sink_valid" internal="sink_valid" />
  <port name="sink_ready" internal="sink_ready" />
  <port name="sink_error" internal="sink_error" />
  <port name="sink_sop" internal="sink_sop" />
  <port name="sink_eop" internal="sink_eop" />
  <port name="sink_real" internal="sink_real" />
  <port name="sink_imag" internal="sink_imag" />
  <port name="inverse" internal="inverse" />
 </interface>
 <interface name="source" internal="fft_ii_0.source" type="conduit" dir="end">
  <port name="source_valid" internal="source_valid" />
  <port name="source_ready" internal="source_ready" />
  <port name="source_error" internal="source_error" />
  <port name="source_sop" internal="source_sop" />
  <port name="source_eop" internal="source_eop" />
  <port name="source_real" internal="source_real" />
  <port name="source_imag" internal="source_imag" />
  <port name="source_exp" internal="source_exp" />
 </interface>
 <module
   name="fft_ii_0"
   kind="altera_fft_ii"
   version="17.0"
   enabled="1"
   autoexport="1">
  <parameter name="data_flow" value="Streaming" />
  <parameter name="data_rep">Block Floating Point</parameter>
  <parameter name="design_env" value="NATIVE" />
  <parameter name="direction" value="Bi-directional" />
  <parameter name="dsp_resource_opt" value="false" />
  <parameter name="engine_arch" value="Quad Output" />
  <parameter name="hard_fp" value="false" />
  <parameter name="hyper_opt" value="false" />
  <parameter name="in_order" value="Natural" />
  <parameter name="in_width" value="16" />
  <parameter name="length" value="1024" />
  <parameter name="num_engines" value="1" />
  <parameter name="out_order" value="Natural" />
  <parameter name="out_width" value="29" />
  <parameter name="selected_device_family" value="Cyclone IV E" />
  <parameter name="twid_width" value="16" />
 </module>
 <interconnectRequirement for="$system" name="qsys_mm.clockCrossingAdapter" value="HANDSHAKE" />
 <interconnectRequirement for="$system" name="qsys_mm.enableEccProtection" value="FALSE" />
 <interconnectRequirement for="$system" name="qsys_mm.insertDefaultSlave" value="FALSE" />
 <interconnectRequirement for="$system" name="qsys_mm.maxAdditionalLatency" value="1" />
</system>
